**static** [**bool**](http://lxr.free-electrons.com/ident?i=bool)[**ip\_exceeds\_mtu**](http://lxr.free-electrons.com/ident?i=ip_exceeds_mtu)**(const struct** [**sk\_buff**](http://lxr.free-electrons.com/ident?i=sk_buff) **\***[**skb**](http://lxr.free-electrons.com/ident?i=skb)**, unsigned int** [**mtu**](http://lxr.free-electrons.com/ident?i=mtu)**)**

This function deals with scenario how to handle when pack exceeds mtu size. So mtu (The Internet's Transmission Control Protocol (TCP) uses the **MTU** to determine the maximum size of each packet in any transmission ) or maximum transmission unit size handling is dealt in this function.